****Invitation to Bid for**

***Repair of RC Deck, Trestle and Fendering System at***

***Port of San Jose, Antique***

1. The *Philippine Ports Authority, PMO-Panay/Guimaras*, through the *PPA Corporate Fund (R/M 2017)* intends to apply the sum of ***Twenty-Eight Million, Three Hundred Twenty-Eight Thousand, One Hundred Eleven Pesos and 62/100 (P28, 328,111.62)*** being the Approved Budget for the Contract (ABC) to payments under the contract for **“*Repair of RC Deck, Trestle and Fendering System at Port of San Jose, Antique” (A170203).*** Bids received in excess of the ABC shall be automatically rejected at bid opening.

The *Philippine Ports Authority, PMO-Panay/Guimaras* now invites bids for:

|  |
| --- |
| * *General Expenses includes pre-con survey, signages and provision of temp. facilities* |
| * *Demolition/removal of rc deck, curtain wall, mooring block and beam.* |
| * *Pile Jacketing* |
| * *Chipping of existing RC piles up to required elevation* |
| * *Supply,deliver and place 3,500 psi concrete pile jacket including forms for built-up and pile jacket.* |
| * *Supply,deliver and place reinforcement for built-up and pile jacket.* |
| * *Construction of RC Deck* |
| * *Supply and place 4,000 psi for RC Deck and rc beam.* |
| * *Steel Reinforcements for Item 5.10* |
| * *Supply and install hot-dipped galvanized 100mm x 100mm x 10mm angle bar for construction and expansion joints including dowel bars* |
| * *Provision of Covered Walkway* |
| * *Demolition/removal of rc walkway, washed and chipping of portion of pavement for retaining wall as shown in the plan* |
| * *Supply and place 4,000 psi for RC walkway deck and rc beam.* |
| * *Supply,deliver and install reinforcements for rc walkway deck and beam* |
| * *Supply and place 3,000 psi PC Concrete for Covered Walkway* |
| * *Plastering/Concrete Finishing Works for an average of 16 mm cement plaster and cement finishing* |
| * *Supply and install steel reinforcement for Item 6.40* |
| * *Supply and install pre-cast RC Trellis as detailed in the plan* |
| * *Supply and install roofing as detailed in the plan* |
| * *Supply and place tile cladding and moulding at column pedestal* |
| * *Supply and install GIP Railing alongside road as detailed in the plancomplete with epoxy primer and epoxy gray top coat paint* |
| * *Painting Works for concrete surface and trellis* |
| * *Mooring System* |
| * *Supply and place 4,000 psi for Mooring Block* |
| * *Supply,deliver and install reinforcements for mooring block* |
| * *Supply, Deliver and Install to site T-Head, 50T mooring bollard incg.accessories* |
| * *Fendering System* |
| * *Performance Test of RDF* |
| * *Supply and place 4,000 psi for RC Fender Block* |
| * *Supply, Fabricate and Install of Steel Reinforcement for item 8.10* |
| * *Supply and Deliver (600H x 2000L) HV-Type Rubber Dock Fenders.* |
| * *Concrete Boring, preparation and placement of SS rod anchor on fender wall* |
| * *Install Rubber Dock Fenders including accessories* |

1. Completion of the Works is required *375 Calendar Days from the effective date of the contract*. Bidders should have completed a contract similar to the Project. The description of an eligible bidder is contained in the Bidding Documents, particularly, in Section II. Instructions to Bidders.
2. Bidding will be conducted through open competitive bidding procedures using non-discretionary “pass/fail” criterion as specified in the 2016 Revised Implementing Rules and Regulations (IRR) of Republic Act 9184 (RA 9184), otherwise known as the “Government Procurement Reform Act.”

Bidding is restricted to Filipino citizens/sole proprietorships, cooperatives, and partnerships or organizations with at least seventy five percent (75%) interest or outstanding capital stock belonging to citizens of the Philippines.

1. Interested bidders may obtain further information from *Engineering Services Division, Philippine Ports Authority, PMO-Panay/Guimaras* and inspect the Bidding Documents at the address given below from ***8:00am to 5:00pm*.**
2. A complete set of Bidding Documents may be acquired by interested bidders starting ***November 14, 2017***from the address below *and upon payment of the applicable fee for the Bidding Documents, pursuant to the latest Guidelines issued by the GPPB, in the amount of* ***Twenty Five Thousand Pesos*** ***(P25, 000.00) VAT Exclusive.***

Itmay also be downloadedfree of charge from the website of the Philippine Government Electronic Procurement System (PhilGEPS) and the website of the Procuring Entity*,* provided that bidders shall pay the applicable fee for the Bidding Documents not later than the submission of their bids.

1. The *Philippine Ports Authority, PMO-Panay/Guimaras* will hold a Pre-Bid Conference on ***November 20, 2017, 10:00 A.M*** at *the* ***PPA Conference Room, 2nd Floor, Admin. Bldg., ICPC, Iloilo City***which shall beopen to prospective bidders.
2. Bids must be duly received by the BAC Secretariat at the address below on or before ***December 4, 2017, 08:30 A.M*** at *the* ***PPA Conference Room, 2nd Floor, Admin. Bldg., ICPC, Iloilo City****.* All bids must be accompanied by a bid security in any of the acceptable forms and in the amount stated in **ITB** Clause 18.

Bid opening shall be on ***December 4, 2017 at 9:00 in the morning*** at *the* ***PPA Conference Room, 2nd Floor, Admin. Bldg., ICPC, Iloilo City****.* Bids will be opened in the presence of the bidders’ representatives who choose to attend at the address below. Late bids shall not be accepted.

1. Other necessary information:

Required Equipments:

|  |
| --- |
| *2- Conc. mixer (1-bagger)* |
| *2- Conc. vibrator (3.5 hp)* |
| *1- Water truck (1,000 gal.)* |
| *1- Stake Truck* |
| *1-Bar cutter (electric, 25mm dia min.)* |
| *2-Bar bender (electric, 25mm dia min.)* |
| *1- Dump truck ( 8 cu.m.)* |
| *2-Oxy/Acetylene cutting outfit* |
| *2-Welding machine* |
| *1-Air compressor (250 cfm)* |
| *1-Jack hammer* |
| *1-Concrete cutter* |
| *1-Backhoe (0.40cu.m., 91hp)* |
| *1-Telescopic Boom Truck, 2~5 tons* |
| *2-Angle Grinder* |
| *2-Steel Circular Saw* |
| *3-Grinder/tile cutter* |
| *2-Sander* |
| *1-Hauling Truck(35T)* |
| *1-Truck Mounted Crane, Telescopic Boom (11-15MT,160Hp)* |
| *2-Concrete Coring machine* |
| *1-Welding Generator (30KVA )* |
| *1- Cargo Truck, 9-10MT,270 Hp* |

* Required PCAB License: Port, Harbor and Offshore Engineering *– Medium A*
* Interested Bidders are advised to bring the original copy of the company’s PCAB Registration and Platinum PhilGeps Registration.

1. The *Philippine Ports Authority, PMO-Panay/Guimaras* reserves the right to reject any and all bids, declare a failure of bidding, or not award the contract at any time prior to contract award in accordance with Section 41 of RA 9184 and its IRR, without thereby incurring any liability to the affected bidder or bidders.
2. For further information, please refer to:

***Engr. Rona Mae B. Barabona***

*BAC Secretariat*

*Philippine Ports Authority, PMO-Panay/Guimaras*

*Brgy. Loboc, Lapaz, Iloilo City*

*(033) 337-7791 local 302-302*

*esd\_pmoiloilo@yahoo.com*

**ANTONIO F. BELARGA**

*Chairperson, BAC-EP*