**FOR THE REPAIR OF GROUTED RIPRAP, RC STAIR, SHEET PILE AND PART OF RC DECK, PORT OF SINDANGAN, ZAMBOANGA DEL NORTE**

The Philippine Ports Authority, PMO- Zamboanga del Norte, through its bids and Awards Committee for Infrastructure Projects intends to apply the sum of **Php 28,838,756.00** being the Approved Budget for the Contract (ABC) to payment under the contract for the **REPAIR OF GROUTED RIPRAP, RC STAIR, SHEET PILE AND PART OF RC DECK, PORT OF SINDANGAN, ZAMBOANGA DEL NORTE**. Bids received in excess of the ABC shall be automatically rejected at Bid Opening.

The PPA, PMO-Zamboanga del Norte, through its Bids and Awards Committee for Infrastructure Projects now invites bids for the project with the following scope of work:

1. **Scope of Work: Quantity**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |  |
| --- | --- | --- |
| **1.00 Mobilization and Demobilization 1.00 LOT**  | **1.00** | **Lot** |
| 2**.00 REPAIR OF GROUTED RIPRAP, RC STAIR**  **AND EXTENSION OF FENCE**  |  |  |
| 2.10 Demolition Works for the Grouted Riprap,RC Stairs,RC 408.00 cu.m curb, pile cap and portion of pavement | 408.00 | **cu.m** |
| 2.20 Excavation and disposal of surplus materials 576.00 cu.m | 576.00 | **cu.m** |
| 2.30 Supply, deliver and place rocks with grout 1,355.00 cu.m |
| 2.40 Supply and install reinforcing steel bars for concrete 30,983.00 kg toppings, concrete curb, pile cap , RC Stairs and fence | 30,983.00 | **kg** |
| 2.50 Supply and place concrete for toppings for riprap, pile 512.00 cu.m cap, RC Stair, Curb, RC Beam, and Extension of CHB Fence |   | **cu.m** |
| 2.60 Masonry Works for the Extension of CHB Fence 12.24 sq.m | 12.24 | **sq.m** |
| 2.70 Steel works for the CHB Fence 667.00 kg |  | 667.00 | **kg** |
| **3.00 REPAIR OF SHEET PILE**  |  |  |  |
| 3.10 Supply and deliver to site 0.35mx0.60m 162.00 In.m RC Sheet Pile, (3,500 psi) | 162.00 | **ln.m** |
| 3.20 Driving of RC Sheet Pile 162.00 In.m |
| 3.30 Supply and install Geotextile Fabric 180.00 sq.m | 180.00 | **sq.m** |
| 4.00 **REPAIR OF RC DECK**   |  |  |  |  |
| 4.10 Falsework for Demolition of RC Deck 234.00 sq.m | 234.00 | **SQ.M** |
| 4.20 Demolition Works for RC Deck 258.00 sq.m |  | 258.00 | **sq.m** |
| 4.30 Rebar Works for RC Deck 29,455.00 kg |
| 4.40 Supply, deliver and install four (4) Units Mooring Bollard 4.00 units | 4.00 | **units** |
| 4.50 Supply and place concrete for RC Deck, 198.00 cu.m RC Beam, Pile Cap and Concrete Curb( 3500 psi ) | 198.00 | **cu.m** |
| **5.00 REPAIR OF PIER APPROACH** |  |  |  |
| 5.10 Demolition and disposal of Existing Concrete Pavement 205.00 sq.m | 205.00 | **sq.m** |
| 5.20 Excavation and disposal of surplus materials for the 270.00 cu.m repair of Pier Approach  | 270.00 | **cu.m** |
| 5.30 Sheating 165.00 sq.m |  | 165.00 | **sq.m** |
| 5.40 Rebar Works for L-Shape Retaining Wall 4,415.00 kg | 4,415.00 | **kg** |
| 5.50 Concreting Works for L-Shape Retaining Wall 27.00 cu.m | 27.00 | **cu.m** |
| 5.60 Rock Works for Pier Approach 222.00 cu.m |  | 222.00 | **cu.m** |
| 5.70 Supply and spread sub base coarse 68.00 cu.m | 68.00 | **cu.m** |
| 5.80 Supply and spread base coarse 68.00 cu.m |  | 68.00 | **cu.m** |
| 5.90 Rebar Works for the restoration and repair of  concrete pavement and concrete drainage. 5,486.00 kg.5.91 Concreting Works for the restoration and  repair of concrete pavement and concrete drainage 63.00 cu.m. | 5,486.00 | **kg** |
| 5.92 Supply and spread hot asphalt for concrete 194.00 In.m pavement contraction joint | 194.00 | **ln.m** |
| 5.93 Repair & Reinstallation of Steel Gratings 21.00 In.m | 21.00 | **ln.m** |
| **6.00 Construction Safety and Health Program 1.00 lot** | **1.00** | **lot** |
|  |  |  |  |  |

 |  |  |  | **1.00** | **Lot** |

1. **Equipment Requirements: Capacity**

|  |
| --- |
| 1-unit Pneumatic Breaker, Hand Held,50ft,Oiler and attach  |
|  1-unit Air Equipment Compressor, Diesel Engine, 130HP  |
| 1-unit Backhoe, wheel mounted ( 0.50 cu.m. cap) 101HP |
|  1-unit Concrete saw 16"-18",Self propelled,6 3/4" cutting depth  |
|  1-unit Dump truck (6-8.99 cu.m) 220 HP  |
| 1-unit Pay loader ( 1.68 cu.m. cap) wheel Type,100hp |
| 1-bagger concrete mixer (4-6cu.ft/min) |
| 1-unit Water truck (cap.500-1000 gals) 360hp |
| 1-unit Rebar Bender up to 25mm,3-phase |
| 1-unit Rebar Cutter 16mm,single-phase |
| 1-unit Transit Mixer 5-6 cu.m cap,175 HP |
| 1-unit Concrete Vibrator 2" |
| 1-unit Welding Machine, AC output, with complete accessories 300 Amp. |
| 1-unit Oxy-Acetylene Cutter w/ complete accessories |
| 1-unit Electric Grinder/Sander |
| 1-unit Crane, all terrain, 246 HP, 45MT cap. |
| 1-unit Drop Hammer with complete pile cap and lead, 2T |
| 1-unit Diesel Pile Hammer (10,500kg-m) |
| 1-unit Guide Rail |
| 1-unit Forklift, capacity 5,000 Lbs |
| 1-unit Chainsaw |
| 1-unitRoad Grader ( 165 HP cap.) |
| 1-unit Road Roller, tandem drum, 118 HP,10.50 tons cap. vibrating  |

Completion of the works is required 276 Calendar Days. Bidders must have an experience of having completed at least one (1) contract that is similar to the contract to be bid, and whose value, adjusted to the current prices, must be at least 50% of the approved budget for the contract to be bid.

Bidding will be conducted through open competitive bidding procedures using non-discretionary pass/fail criterion as specified in the Implementing Rules and Regulations of Republic Act 9184 (RA 9184), otherwise known as the “Government Procurement Reform Act”.

Bidding is restricted to Filipino citizens/Sole proprietorships, partnerships, or organizations with at least seventy five percent (75%) interest or outstanding capital stock belonging to citizens of the Philippines and with Minimum PCAB License Registration-Medium A- Ports, Harbor and Offshore Engineering.

Interested bidders may obtain further information from PPA, PMO-Zamboanga del Norte and inspect the Bidding Documents at the address given below from 8:00AM to 5:00PM, Monday to Friday.

Letter of Intent will be received from July 12-18, 2017. Only Letter of Intent (LOI) with attached 1- xerox copy of PCAB License and required experience will be accepted. Please present Original Copy of PCAB License at the time of submission of LOI for verification purposes. Bidders without similar experience to the contract to be bid need not apply.

A complete set of Bidding Documents may be purchased by interested bidders from the address below and upon payment of a non-refundable fee for the Bidding Documents in the amount of Twenty Five Thousand Pesos (Php 25,000.00), exclusive of VAT.

The PPA, PMO-Zamboanga del Norte will hold a Pre-Bid conference on July 19, 2017, 10:00 AM at PPA Conference Room, Admin. Bldg., Port of Dapitan, Dapitan City, ZDN, which shall be open only to all interested parties who have purchased the Bidding Documents.

Bids must be delivered to the address below on or before August 1, 2017, 10:00 AM at PPA Conference Room, PMO-Zamboanga del Norte, Port area, Dapitan City address to the BAC Chairman for Infrastructure Projects. All bids must be accompanied by a bid security in any of the acceptable forms and in the amount stated in the Instruction to Bidders. Bids will be opened in the presence of the bidder’s representatives who choose to attend at the address below. Late bids shall not be accepted.

The PPA, PMO-Zamboanga del Norte reserves the right to accept or reject any bid, to annul the bidding process, and to reject all bids at any time prior to contract award, without thereby incurring any liability to the affected bidder or bidders.

**(SGD)ENGR. ABDURASAD S. HASAN**

BAC Chairperson for Infrastructure Projects

PPA, PMO-Zamboanga del Norte, Port Area, Dapitan City 7101

For further information, please refer to:

The BAC Secretariat for Infrastructure Projects or The ESD Office

PPA, PMO-Zamboanga del Norte, Port Area, Dapitan City 7101

Tel No. (065) 213-6595, (065) 213-6946

Email Address:ppa.pmo.dapitan@gmail.com

Date of Publication: July 12-18, 2017

PPA Website: www.ppa.com.ph

PhilGeps Website: www.philgeps.net

Philippine Star (Newspaper) July 12, 2017